* **Folder Robo\_Keypad\_PCB**
  + Use the latest version as labeled by the folder name, currently being “v1.2”.
  + The files need to access using Autodesk Eagle software.
* **Folder Keypad\_Code**
  + The file Keypad\_Main.ino is the main file and can be opened using Arduino IDE and flashed onto the keypad control board (ESP32 on the keypad)
  + The other files are dependencies of the main file.
* **Folder CAD Files**
  + The files in this folder include CAD files for the covers of the keypad.
  + The .step and .f3d are editable files that can be opened and edited using Fusion360 software.
  + The two other .stl files (Keypad\_UP\_Cover and Keypad\_D\_Cover) are files used for 3D printing the cover for the keypad.